(footprint "A768X-EC800M-FP"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at -10.4 -2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(property "Value" "A768X-EC800M-FP"
		(at 0 1 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" "A768X-EC800M-FP"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr through_hole)
	(fp_line
		(start -23.495 -7.874)
		(end 1.4224 -7.874)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start -23.495 15.24)
		(end -23.495 -7.874)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.4224 -7.874)
		(end 1.4224 15.24)
		(layer "Edge.Cuts")
	)
	(fp_line
		(start 1.4224 15.24)
		(end -23.495 15.24)
		(layer "Edge.Cuts")
	)
	(fp_text user "RI"
		(at -2.95 0.55 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "DTR"
		(at -2.95 2.95 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "ANT"
		(at -20.65 -2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "RXD"
		(at -20.5 5.55 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "MICP"
		(at -3.1 5.45 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SPKP"
		(at -3.15 10.65 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "VCC\n"
		(at -20.55 0.5 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "MICN"
		(at -3.15 8.1 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "SPKN"
		(at -3.2 13.2 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "RST"
		(at -20.55 3.1 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "GND"
		(at -20.45 10.7 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "TXD"
		(at -20.5 8 0)
		(unlocked yes)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0 2.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "" np_thru_hole circle
		(at -21.7236 13.576)
		(size 2 2)
		(drill 2)
		(layers "*.Cu" "*.Mask")
	)
	(pad "1" thru_hole rect
		(at -22.0736 -2.524)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "1" thru_hole rect
		(at 0 0)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at -22.0736 0.016)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "2" thru_hole oval
		(at 0 2.54)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at -22.0736 2.556)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "3" thru_hole oval
		(at 0 5.08)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at -22.0736 5.096)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "4" thru_hole oval
		(at 0 7.62)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at -22.0736 7.636)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "5" thru_hole oval
		(at 0 10.16)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at -22.0736 10.176)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(pad "6" thru_hole oval
		(at 0 12.7)
		(size 1.7 1.7)
		(drill 1)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
	)
	(model "${KIPRJMOD}/TDM-4G-V1-3D.STEP"
		(offset
			(xyz -21.75 -13.55 2.5)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)
